**Open Lab 2**

**Digital Communication**

Question 1:

Estimate value of Eb/No required to pass 8-QAM modulated signal through single tap Rayleigh Channel while keeping BER 1e-3 at max.

Repeat for 8-PSK. Is there a difference in the two values? Explain your findings.